Figure 6: Peripheral Controlers